| ### TI Connect Manager X Scripting Interface Documentation |
Apple Event Device Clock Status Enumerations | 4-Char ID |
clock on - the device clock is currently enabled (status), or the device clock will be turned on when the clock record is sent to the device. | kCKo |
clock off - the device clock is currently disabled (status), or the device clock will be turned off when the clock record is sent to the device. | kCKf |
clock same - the device clock will be left in the same state as it is in currently, when the clock record is sent to the device. | kCKs |
BACK | 12 March 2003 - slr |