| ### TI Connect Manager X Scripting Interface Documentation |
Apple Event Login Status Enumerations | 4-Char ID |
login pending - the application is waiting for the login sequence from the specified device. This can be either a status, or a value passed to set the application to wait for login from the specified device (ie. using the set event rather than the login event). | eLPn |
logged in - the specified device is currently "logged in", and the name the user typed into the LOGIN app is available in the device login name property. | eLgI |
not logged in - the specified device is not currently logged in. | eLnI |
BACK | 12 March 2003 - slr |