| ### TI Connect Manager X Scripting Interface Documentation |
Apple Event Application Properties and Elements | 4-Char ID |
name - the name, in Unicode text, of the application. [ro] [ utxt ] (property) | pnam |
version - the version information (number) of the application [ro] [ vers ] (property) | vers |
supported models - the list of supported device model identifiers currently supported by this version of the application. [ro] [ constant ] (property) | pSMo |
supported devices - the list of supported device model names, in Unicode Text, currently supported by this version of the application. [ro] [ utxt ] (property) | pSDe |
usb suspend delay - the number of seconds of inactivity on a direct USB-connected device before the USB port segment is suspended [ integer ] (property) { note this property has a granularity of 4 seconds } | pSDt |
usb resume delay - - the number of milli-seconds of resume-delay on a direct USB-connected device before a USB error is indicated in the event the device does not properly respond to a resume signal [ integer ] (property) | pRDt |
resolution - - the dpi (dots per inch) resolution to be used when converting screen shots and picture objects to the typePict ('PICT') format. [ constant ] (property) | pReS |
device - a TI educational device, by ID or name or index (element) | cEDv |
unknown device - a TI educational device, by ID or name or index that has not yet been identified, or cannot be identified. (element) | cUED |
active device - a TI educational device, by ID or name or index, that may be currently in use performing communication. This element is used to acquire status information about the current specified device. (element) | cIED |
Key Form support
form Absolute Position | indx
form Test | test
form Name | name
form Relative Position | rele
by ID number value (not with unknown device(s)) | 'ID '
form Property ID * (unknown device only) | prop
BACK | 04 December 2004- slr |