| ### TI Connect Manager X Scripting Interface Documentation |
set reference to anything | core : setd |
The set command is used to set application-specific properties, and can be used to send data to an attached device. Generally, the SEND command is better for this latter process however. Examples of using this event are: set contents of file 1 of device 1 to somedata set model of unknown device 3 to TI83Plus SE set user name of device 1 to "My Very Own Device" set directory filter of device 1 to TI92Plus application variable set usb suspend delay to 16 The reply to this event is a numeric long value, representing the error status of the operation. |
BACK | 01 March 2004 - slr |