| ### TI Connect Manager X Scripting Interface Documentation |
Apple Event Enumerations | ID |
Content Type - used in Directory Item records | cTyp |
Battery Level - used in device battery properties | cBat |
TI Device classes - used in device model properties | cTIC |
Object Flags - used in Directory Item records | cFlg |
TI Device features - used in device feature properties | cFea |
TI Device Family - used in device family properties | cFam |
Object Location indicator - used in SEND events to provide an override capability to the object being sent default destination ( either RAM, or Archive, and locked or not) | cLoc |
Object Name status - used in Response record for Check Name event | cSta |
TI Device Login Status - used in device logged in properties | cLog |
Directory Filter - used to set directory filter value in set property event. This is a key descriptor value. Use the device data type classes to specify the filter value. | cFlt |
Clock State - used in clock record to set device clock state, and returned in clock record to indicate current device clock state | cDcs |
I/O Progress State - used in retrieving I/O progress information on active devices. | eIOs |
Connection - used to specify how the device is connected or interfaced to the computer | cCon |
BACK | 01 March 2004- slr |