| ### TI Connect Manager X Scripting Interface Documentation |
send reference to reference [ in type class ] | TIco : TIsd |
This script command informs TI Connect Manager X to send the specified data object(s) to the specified device, storing the data in either RAM (default), or archive, or optionally as a locked item in RAM. Examples of using this event are: send a to device 1 send contents of file "file:///test.9xk" to device named "Steve's TI-92" send b to (every device where model is TI83Plus) in archive The reply to this event is a descriptor containing a (possibly list of) value(s) where a value of zero means the object was sent properly, and non-zero indicates a specific error condition on the sending of the object. |
BACK | 9 April 2003 - slr |