| ### TI Connect Manager X Scripting Interface Documentation |
Apple Event Object Clock Record properties | 4-Char ID |
device date - date and time currently available on device or date and time to set on device. [ 'ldt ' ]. | pDAT |
time zone - time zone in hours from GMT [ 'long' ] | pDtz |
date format - format to use in reprensting date (device specific, from 1 to n, where n is the number of elements in the list returned for the date setting property). [ 'long' ] | pDdf |
date setting - on getting the clock from the device, this contains a list of unicode formatted strings representing the settings for the date format above. [ 'utxt' ] | pDtS |
time format - format to use in representing clock time on device (12- or 24- hour format). [ 'long' ] | pDtf |
state - clock state (on, off, same). [ 'cDcs' ] | pDcs |
BACK | 01 March 2004 - slr |