| ### TI Connect Manager X Scripting Interface Documentation |
Apple Event TI Device Class Definitions | Class ID |
best type | best |
TI82 device | FF82FFFF |
TI73 device | FF74FFFF |
TI83 device | FF83FFFF |
TI83plus device (covers TI83 Plus Silver, TI84 Plus and TI84 Plus Silver) | FF73FFFF |
TI85 device | FF85FFFF |
TI86 device | FF86FFFF |
TI89 device (covers TI-89 Titanium) | FF98FFFF |
TI92 device | FF89FFFF |
TI92plus device (covers Voyage 200) | FF88FFFF |
CBL device | FF41FFFF |
CBL2 device | FF42FFFF |
CBR device | FF16FFFF |
TI Presenter device | FF43FFFF |
USB-connected (CARS) device | n/a |
Device-data Localization | n/a |
BACK | 04 March 2004 - slr |