| ### TI Connect Manager X Scripting Interface Documentation |
Apple Event Object Connection Enumerations | 4-Char ID |
TI Connectivity Cable USB - connection to device is via the "silver" TI USB interface cable. | eSil |
Direct USB - connection to the device is via a "direct" USB connection (such as available on devices in the TI-84Plus family). | eCAR |
Navigator Network - connection is via an access point to a TI-Navigator Network | eNav |
BACK | 01 March 2004 - slr |