| ### TI Connect Manager X Scripting Interface Documentation |
Apple Event Device Features Enumerations | 4-Char ID |
supports request - device supports device request operation | eRDC |
supports zero request - device supports device request operation with a device identifier of zero | eZer |
product loaded - device currently has product operating system code loaded | eOSl |
device busy - device is currently busy | eBsy |
supports info - device supports the request device information operation | eRDI |
supports flash - device has, and supports, flash memory operations | eFls |
supports filtered directory - device supports retrieval of directory information that can be pre-filtered by the device | eFlt |
device home - device is currently on the "home" screen and it is safe to communicate in all modes | eHom |
supports clock - the device has, and supports, real-time clock operations | eClk |
supports archive - the device has the ability to store items in archive | eARc |
supports screen - the device has a display and supports the retrieval of the display contents | eScb |
supports login - the device has the "LOGIN" app loaded and supports the login protocol | eLgn |
supports folders - the device has a built-in folder structure | eFld |
supports delete - the device supports the deletion of items via the link | eDel |
supports apps - the device supports the concept of applications | eAps |
supports login - the device has the LOGIN app loaded and supports login | eLgn |
supports keys - the device has the ability to be remote-controlled via sending key-presses on the link. | eKey |
BACK | 12 April 2004- slr |