| ### TI Connect Manager X Scripting Interface Documentation |
Apple Event Device Family Enumerations | 4-Char ID |
other family - device does not belong to a specific family of devices; currently includes the TI-82, CBR, TI-Presenter and original CBL | OtFa |
TI83 family - device is one of TI-83, TI-83Plus, TI-83Plus SE, or TI-73. The TI-82 is NOT in this family since some of it data types are not compatible with the 83 class of device. The TI-84Plus family of devices is included in this family. | 83Fa |
TI85 family - device is one of TI-85 or TI-86. | 85Fa |
TI92 family - device is one of TI-92, TI-89, TI-92Plus, or Voyage 200, or TI-89 Titanium. | 92Fa |
CBL family - device is either a CBL 2 or LabPro device | C2Fa |
BACK | 12 April 2004 - slr |