Home
You are here: Introduction to TI Device Explorer > Working with Distribution Lists > Using error distribution lists

## Using error distribution lists

TI Device Explorer creates an error distribution list when an error occurs during a send operation. TI Device Explorer names the error distribution list based on the file that did not send correctly. In the error distribution list, you can find all of the devices to which the software did not send the file. You can then use the error distribution list to resend the file once you resolve the problem that caused the send failure.

Notes:

| • | Although the error distribution list is named based on the sent file, it does not contain the file.

| • | You cannot edit or intentionally create an error distribution list.

### To use error distribution lists

| 1. | Resolve the error that caused the software to not send the file.

Note: You can determine the error using the history window. Click Window > History and locate the explanation for why the send failed.

| 2. | If the distribution list drawer is not open, click View > Toggle Distribution List Drawer or click Distribution Lists.

| 3. | Click the error distribution list for the file you want to resend.

The main window displays the devices to which the software did not send the file.

| 4. | Select the devices.

| 5. | Resend the file. (See "Sending files to connected devices".)

© 2005 - 2013 Texas Instruments Incorporated