| ### TI Connect Manager X Scripting Interface Documentation |
Apple Event Unknown Device key field descriptors | 4-Char ID |
name - in Unicode text format [ 'utxt' ] | pnam | container
size - of object, in bytes [ 'long' ] | ptsz
class - type class of object for target device [ 'type' ] | pcls
model - model descriptor of this particular device [ 'cTIC' ] | pMod |
id - device serial number (unique for any devices with serial numbers built-in) [ 'ctxt' ] | ID |
battery - enumeration indicating current battery status. [ 'cBat' ] | pBat |
cable name - name of cable of port location id. [ 'ctxt' ] | pCnm |
features - supported device feature information for this device [ 'cFea' ] | feat |
user name - in Unicode text format, the current user name for this device [ 'utxt' ] | pUNm |
Key Form support
form Absolute Position | indx
form Test | test
form Name | name
form Relative Position | rele
form property ID | prop
BACK | 12 April 2004- slr |