| ### TI Connect Manager X Scripting Interface Documentation |
Apple Event Object Product Record properties | 4-Char ID |
OS revision - revision level of the current OS present on the device [ 'doub' ]. | pOSr |
Rom revision - current level of ROM code present on device (sometimes referred to as "boot" or "shadow boot" code.) [ 'doub' ] | pRMr |
hardware revision - device and model-specific hardware version information. [ 'long' ] | pHWr |
active language - current selected language code for device. [ 'doub' ] | pLGr |
product id - product-family specific identification number of this device. [ 'long' ] | pPID |
BACK | 01 March 2004 - slr |