| ### TI Connect Manager X Scripting Interface Documentation |
login reference | TIco : TIli |
This script command informs TI Connect Manager X to wait for a login message from the referenced device. Examples of using this event are: login device 1 with timeout of 60 seconds login device 1 end with This event activates a "listener" that monitors communications from the device and waits for a "login" response. The reply to this event is a yes/no response of whether or not the device logged in, or a timeout error if the login process timed out without logging in. Default period is 30 seconds for login before timeout, which can be adjusted using the with clause. |
BACK | 18 March 2004 - slr |