| ### TI Connect Manager X Scripting Interface Documentation |
Apple Event Terminology | Event Class : ID |
count reference [ each type class ] | core : cnte |
data size reference [ as type class ] | core : dsiz |
data version reference [ as type class ] | TIco : TIdv |
delete reference | core : delo |
exists reference | core : doex |
get reference [ as [a list of] type class ] | TIco : getd |
open reference | aevt : odoc |
quit | aevt : quit |
save reference [ in alias ] [ as type class ] [ with replacing ] | core : save |
set reference to anything | core : setd |
send reference to reference [ in type class ] | TIco : TIsd |
enable notification [ reference ] | TIco : TIno |
disable notification | TIco : TInf |
notifications enabled | TIco : TIne |
reacquire reference | TIco : TIrd |
refresh reference | TIco : TIrf |
coerce anything as [a list of] type class | TIco : ktra |
disable identification reference | TIco : TIdi |
wait for reference from reference [ as [a list of] type class ] | TIco : TIwf |
check name reference as [a list of] type class | TIco : TIcn |
sendkey integer to reference [ capturing screen true/false ] [ delaying integer ] [ capturing color screen true/false ] | TIco : TIsk |
login reference | TIco : TIli |
terminate integer | TIco : TIte |
reopen | aevt : rapp |
device added reference * | TIco : TIda |
device removed reference * | TIco : TIdr |
device logged in reference * | TIco : TIlo |
device login timedout reference * | TIco : TIdt |
BACK | 18 March 2004 - slr |
| * - events marked as such are notification events sent FROM the TI Connect Manager X to client-applications that have registered via the enable notifications event. |